| gclib 1.32.6 Communications API for Galil controllers and PLCs |

record_position.cpp
Go to the documentation of this file.
1
8 #include "examples.h"
9
10 #include <iostream> //std::cout
11 #include <fstream>
12
13 #define G_LASTINDEX 999
14
15 using namespace std;
16
17 void write_array_to_file(GCon g, ofstream& os, const char* array_name,
18 int previous_rd, int rd);
19
20 GReturn record_position(GCon g, char* fileA, char* fileB)
21 {
22 ofstream osA, osB;
23 osA.open(fileA, ios::out | ios::trunc);
24 osB.open(fileB, ios::out | ios::trunc);
25
26 int recording = 1;
27
28 e(GProgramDownload(g,
29 "RC 0;' Disable Recording\n"
30 "DP 0, 0;' Set current position to 0\r"
31 "DM posA[1000], posB[1000];' Define a new array that will hold positional data\r"
32 "RA posA[], posB[];' Sets position array to be where recorded data will be stored\r"
33 "RD _TPA, _TPB;' Defines Position to be the type of data that will be recorded\r"
34 "RC 1,-1000;' Begins recording at 512Hz in continuous mode\r"
35 "MO AB;' Turns motors off\r"
36 "AI -1;' Waits for active low on Input 1\r"
37 "RC 0;' Disable Recording after Input 1 goes low\r"
38 "EN;' End program", 0));
39 e(GCmd(g, "XQ")); //Begins execution of program
40
41 int rd = 0;
42 int previous_rd = 0;
43
44 do
45 {
46 GSleep(1000); //Sleep while we wait for roughly half the array to be written
47 e(GCmdI(g, "MG _RD", &rd)); //Gets address of next value in the position array
48
49 //Get values from posA[] array and write to file
50 write_array_to_file(g, osA, "posA[]", previous_rd, rd);
51
52 //Get values from posB[] array and write to file
53 write_array_to_file(g, osB, "posB[]", previous_rd, rd);
54
55 e(GCmdI(g, "MG _RC", &recording)); // Check status of RC
56
57 previous_rd = rd;
58 } while (recording); //While recording is active
59
60 osA.close();
61 osB.close();
62
63 return GALIL_EXAMPLE_OK;
64 }
65
67 void write_array_to_file(GCon g, ofstream& os, const char* array_name,
68 int previous_rd, int rd)
69 {
70 char buf[G_HUGE_BUFFER]; //traffic buffer
71
72 if (previous_rd < rd) // No array wrap around
73 {
74 e(GArrayUpload(g, array_name, previous_rd, rd - 1, G_COMMA, buf, G_HUGE_BUFFER));
75 os << ',' << buf;
76 }
77 else // Array wrapped around - grab two separate chunks from the array
78 {
79 e(GArrayUpload(g, array_name, previous_rd, G_LASTINDEX, G_COMMA, buf, G_HUGE_BUFFER));
80 os << ',' << buf;
81
82 if (rd != 0)
83 {
84 e(GArrayUpload(g, array_name, 0, rd - 1, G_COMMA, buf, G_HUGE_BUFFER));
85 os << ',' << buf;
86 }
87 }
88 }
examples.h
GSleep
GCLIB_DLL_EXPORTED void GCALL GSleep(unsigned int timeout_ms)
Uses GUtility() and G_UTIL_SLEEP to provide a blocking sleep call which can be useful for timing-base...
Definition: gclibo.c:24
GCmdI
GCLIB_DLL_EXPORTED GReturn GCALL GCmdI(GCon g, GCStringIn command, int *value)
Wrapper around GCommand that provides the return value of a command parsed into an int.
Definition: gclibo.c:278
GProgramDownload
GCLIB_DLL_EXPORTED GReturn GCALL GProgramDownload(GCon g, GCStringIn program, GCStringIn preprocessor)
Downloads a program to the controller's program buffer.
GCmd
GCLIB_DLL_EXPORTED GReturn GCALL GCmd(GCon g, GCStringIn command)
Wrapper around GCommand for use when the return value is not desired.
Definition: gclibo.c:237
GArrayUpload
GCLIB_DLL_EXPORTED GReturn GCALL GArrayUpload(GCon g, const GCStringIn array_name, GOption first, GOption last, GOption delim, GBufOut buffer, GSize buffer_len)
Uploads array data from the controller's array table.
G_COMMA
#define G_COMMA
For GArrayUpload(), use this value in the delim field to delimit with commas.
Definition: gclib.h:54
GReturn
int GReturn
Every function returns a value of type GReturn. See gclib_errors.h for possible values.
Definition: gclib.h:93
G_HUGE_BUFFER
#define G_HUGE_BUFFER
Most reads from Galil hardware are small. This value will hold the largest array or program upload/do...
Definition: gclib.h:90
GCon
void * GCon
Connection handle. Unique for each connection in process. Assigned a non-zero value in GOpen().
Definition: gclib.h:94
e
void e(GReturn rc)
A trivial, C++ style return code check used in Galil's examples and demos.
Definition: examples.h:33
record_position
GReturn record_position(GCon g, char *fileA, char *fileB)
Record user's training and saves to a text file.
Definition: record_position.cpp:20
write_array_to_file
void write_array_to_file(GCon g, ofstream &os, const char *array_name, int previous_rd, int rd)
Grabs data from array on controller and writes it to the given text file.
Definition: record_position.cpp:67