| gclib 1.34.15 Communications API for Galil controllers and PLCs |

motion_complete.cpp
Go to the documentation of this file.
1
10 #include "examples.h"
11
12 #include <iostream> //std::cout
13 #include <string.h>
14 using namespace std;
15
16 int check_interrupts(GCon g, GCStringIn axes);
17
18 GReturn motion_complete(GCon g)
19 {
20 char* trimmed;
21
22 cout << "\n*************************************************************\n";
23 cout << "Example GInterrupt() usage\n";
24 cout << "***************************************************************\n";
25
26 char buf[G_SMALL_BUFFER]; //traffic buffer
27 GSize bytes_read;
28
29 //-------------------------------------------------------------------------
30 //simple check for appropriate communication bus
31 //EI will fail below if interrupts are not supported at all
32 bool ei_support = true;
33 if (GCommand(g, "WH", buf, G_SMALL_BUFFER, &bytes_read) == G_NO_ERROR)
34 {
35 //for this example, assume Ethernet connections supports interrupts.
36 ei_support = (strstr(buf, "IH") != 0);
37 }//else assume PCI supports
38
39 if (!ei_support)
40 {
41 cout << "No support on this bus\n";
42 return G_UNSUPPORTED_FUNCTION;
43 }
44
45 //-------------------------------------------------------------------------
46 //Flush interrupts
47 e(GCmd(g, "EI0,0")); //turn off interrupts
48 GStatus status;
49 e(GTimeout(g, 0)); //zero timeout
50
51 //flush interrupts, status will be zero when queue is empty
52 while ((GInterrupt(g, &status) == G_NO_ERROR) && status);
53 e(GTimeout(g, -1)); //restore timeout
54
55
56 //-------------------------------------------------------------------------
57 // Independent motion
58 e(GCmd(g, "DP 0,0")); //define position zero on A and B
59 e(GCmdT(g, "RP", buf, G_SMALL_BUFFER, &trimmed));
60 cout << "\nPosition: " << trimmed << '\n';
61 e(GCmd(g, "SP 4000,4000")); //set up speed
62 e(GCmd(g, "AC 1280000,1280000")); //acceleration
63 e(GCmd(g, "DC 1280000,1280000")); //deceleration
64 e(GCmd(g, "PR 8000,10000")); //Postion Relative. B will take longer to make its move.
65 e(GCmd(g, "SH AB")); //Servo Here
66 cout << "Beginning independent motion...\n";
67 e(GCmd(g, "BG AB")); //Begin motion
68 check_interrupts(g, "AB"); //Block until motion is complete on axes A and B
69 cout << "Motion Complete on A and B\n";
70 e(GCmdT(g, "RP", buf, G_SMALL_BUFFER, &trimmed));
71 cout << "Position: " << trimmed << '\n';
72
73 return GALIL_EXAMPLE_OK;
74 }
75
77 int check_interrupts(GCon g, GCStringIn axes)
78 {
79 char buf[G_SMALL_BUFFER]; //traffic buffer
80 GReturn rc;
81 GStatus status;
82 //bit mask of running axes, axes arg is trusted to provide running axes.
83 //Low bit indicates running.
84 unsigned char axis_mask = 0xFF;
85
86 int len = strlen(axes);
87 //iterate through all chars in axes to make the axis mask
88 for (int i = 0; i < len; i++)
89 {
90 //support just A-H
91 switch (axes[i])
92 {
93 case 'A':
94 axis_mask &= 0xFE;
95 break;
96 case 'B':
97 axis_mask &= 0xFD;
98 break;
99 case 'C':
100 axis_mask &= 0xFB;
101 break;
102 case 'D':
103 axis_mask &= 0xF7;
104 break;
105 case 'E':
106 axis_mask &= 0xEF;
107 break;
108 case 'F':
109 axis_mask &= 0xDF;
110 break;
111 case 'G':
112 axis_mask &= 0xBF;
113 break;
114 case 'H':
115 axis_mask &= 0x7F;
116 break;
117 }
118 }
119 sprintf(buf, "EI %u", (unsigned char)~axis_mask);
120 e(GCmd(g, buf)); //send EI axis mask to set up interrupt events.
121
122 while (axis_mask != 0xFF) //wait for all interrupts to come in
123 {
124 if ((rc = GInterrupt(g, &status)) == G_NO_ERROR)
125 {
126 switch (status)
127 {
128 case 0xD0: //Axis A complete
129 axis_mask |= 0x01;
130 break;
131 case 0xD1: //Axis B complete
132 axis_mask |= 0x02;
133 break;
134 case 0xD2: //Axis C complete
135 axis_mask |= 0x04;
136 break;
137 case 0xD3: //Axis D complete
138 axis_mask |= 0x08;
139 break;
140 case 0xD4: //Axis E complete
141 axis_mask |= 0x10;
142 break;
143 case 0xD5: //Axis F complete
144 axis_mask |= 0x20;
145 break;
146 case 0xD6: //Axis G complete
147 axis_mask |= 0x40;
148 break;
149 case 0xD7: //Axis H complete
150 axis_mask |= 0x80;
151 break;
152 }
153 }
154 }
155
156 return rc;
157 }
examples.h
GCmdT
GCLIB_DLL_EXPORTED GReturn GCALL GCmdT(GCon g, GCStringIn command, GCStringOut trimmed_response, GSize response_len, GCStringOut *front)
Wrapper around GCommand that trims the response.
Definition: gclibo.c:243
GTimeout
GCLIB_DLL_EXPORTED GReturn GCALL GTimeout(GCon g, short timeout_ms)
Uses GUtility() and G_UTIL_TIMEOUT_OVERRIDE to set the library timeout.
Definition: gclibo.c:65
GCommand
GCLIB_DLL_EXPORTED GReturn GCALL GCommand(GCon g, GCStringIn command, GBufOut buffer, GSize buffer_len, GSize *bytes_returned)
Performs a command-and-response transaction on the connection.
GInterrupt
GCLIB_DLL_EXPORTED GReturn GCALL GInterrupt(GCon g, GStatus *status_byte)
Provides access to PCI and UDP interrupts from the controller.
GCmd
GCLIB_DLL_EXPORTED GReturn GCALL GCmd(GCon g, GCStringIn command)
Wrapper around GCommand for use when the return value is not desired.
Definition: gclibo.c:237
GReturn
int GReturn
Every function returns a value of type GReturn. See gclib_errors.h for possible values.
Definition: gclib.h:93
G_SMALL_BUFFER
#define G_SMALL_BUFFER
Most reads from Galil are small. This value will easily hold most, e.g. TH, TZ, etc.
Definition: gclib.h:89
GStatus
unsigned char GStatus
Interrupt status byte.
Definition: gclib.h:101
G_NO_ERROR
#define G_NO_ERROR
Return value if function succeeded.
Definition: gclib_errors.h:13
GSize
unsigned int GSize
Size of buffers, etc.
Definition: gclib.h:95
GCon
void * GCon
Connection handle. Unique for each connection in process. Assigned a non-zero value in GOpen().
Definition: gclib.h:94
G_UNSUPPORTED_FUNCTION
#define G_UNSUPPORTED_FUNCTION
Function cannot be called on this bus. E.G. GInterrupt() on serial.
Definition: gclib_errors.h:52
GCStringIn
const char * GCStringIn
C-string input to the library. Implies null-termination.
Definition: gclib.h:98
e
void e(GReturn rc)
A trivial, C++ style return code check used in Galil's examples and demos.
Definition: examples.h:33
motion_complete
GReturn motion_complete(GCon g)
Uses interrupts to track when the motion of controller is completed.
Definition: motion_complete.cpp:18
check_interrupts
int check_interrupts(GCon g, GCStringIn axes)
Monitors interrupt status on the given axes and returns when interrupts are fired.
Definition: motion_complete.cpp:77