| gclib 1.35.5 Communications API for Galil controllers and PLCs |

Message Example

C++ | C# | Visual Basic
--- | --- | ---
Example | Example | Example
Logic | Logic | Logic
Instructions | Instructions | Instructions

We are always interested in what our customers would like to see! To request any new examples or supported languages, please email suppo.nosp@m.rt@g.nosp@m.alil..nosp@m.com.

## Concepts

This example demonstrates:

- How to connect to a controller via IP Address.
- How to issue basic commands.
- How to reconstitute a full message from GMessage().
- How to detect differences in crashed DMC code and Trace.
- How to print messages.
- How to use Keep Alive to maintain connection to gcaps.

## Prerequisites

A Galil controller with a motor connected at the A axis is needed for this example.

## Command Line Arguments

This example requires 1 argument:

- The IP Address of a Galil controller.

message_example.exe 192.168.42.96

## Example Output

`************************************************************************`
Example GMessage() usage
`************************************************************************`
<HELLO WORLD
>
Trace Line: 0 i=0
Trace Line: 1 #A
Trace Line: 2 MGi
Standard Line: 0.0000
Trace Line: 3 i=i+1
Trace Line: 4 WT100
Trace Line: 5 JP#A,i<1
Trace Line: 6 i=i/0
Crashed Code: ?6 i=i/0