| gclib 2.0.7 Communications API for Galil controllers and PLCs |

## ◆ GInterrupt()

byte GInterrupt | ( |  | ) |
| inline

Provides access to PCI and UDP interrupts from the controller.

Returns
  The status byte from the controller. Zero will be returned if a status byte is not read.

Wrapper around gclib GInterrupt(), http://www.galil.com/sw/pub/all/doc/gclib/html/gclib_8h.html#a5bcf802404a96343e7593d247b67f132 -s ALL or -s EI must be specified in the address argument of GOpen() to receive interrupts.

Definition at line 364 of file gclib.cs.

Referenced by Examples.Motion_Complete().