| gclib 2.0.7 Communications API for Galil controllers and PLCs |

## ◆ x_dr_motioncomplete()

int x_dr_motioncomplete | ( | GCon | g,
|  | GCStringIn | axes
| ) |  |

Example of MotionComplete with data records.

Uses axis status in data record to determine when motion has completed.

Parameters

  g | Connection's handle.
  axes | Mult-axis mask for determining motion complete. ABCDEFGH valid.

Definition at line 92 of file x_grecord.cpp.