| gclib 2.0.7 Communications API for Galil controllers and PLCs |

## ◆ x_ei_motioncomplete()

int x_ei_motioncomplete | ( | GCon | g,
|  | GCStringIn | axes
| ) |  |

Example of MotionComplete with interrupts.

Uses motion complete status bytes to determine when motion has completed.

Parameters

  g | Connection's handle.
  axes | Mult-axis mask for determining motion complete. ABCDEFGH valid. Axes must be in motion when function is called.

Definition at line 85 of file x_ginterrupt.cpp.