| gclib 450 Communications API for Galil controllers and PLCs |

Installation

gclib is available on the following operating systems.

- Microsoft Windows
  - 10 x64 ♦, x86
  - 8.1 x64 ♦, x86
  - 8 x64 ♦, x86
  - 7 x64 ♦, x86
- Ubuntu Linux
  - 18.04 LTS x64 ♦
  - 16.04 LTS x64 ♦ †
  - 14.04 LTS x64 †
  - 12.04 LTS x64 †
- Fedora Linux
  - fc30 x64 ♦
  - fc29 x64 ♦ †
  - fc28 x64 ♦ †
  - fc27 x64 ♦ †
  - fc26 x64 ♦ †
  - fc25 x64 ♦ †
  - fc24 x64 ♦ †
  - fc23 x64 ♦ †
  - fc22 x64 †
  - fc21 x64 †
- Red Hat and CentOS
  - Red Hat 7 & CentOS 7 Linux
    - RHEL 7 x64 ♦
    - CentOS 7 x64 ♦
  - Red Hat 6 & CentOS 6 Linux
    - RHEL 6 x64 †
    - CentOS 6 x64 †
- Raspbian, Raspberry Pi
  - Raspberry Pi 3 Model B+, Stretch 9.8
  - Raspberry Pi 3 Model B, Stretch 9.1 †
  - Raspberry Pi 2 Model B, Jessie 8.0 †
- Apple OS X
  - Yosemite 10.10 x64
  - Mavericks 10.9 x64
- Other builds, contact Galil Applications for more info
  - Nvidia Jetson TX1 running Ubuntu 16.04 arm64

♦ gcaps available on these operating systems.

† Although no longer built on these older operating systems, previous versions of gclib are available.

Don't see your OS? Please email softw.nosp@m.ares.nosp@m.uppor.nosp@m.t@ga.nosp@m.lil.c.nosp@m.om, or call Galil Applications.