| gclib 2.4.1 Galil Communications Library

Loading...
Searching...
No Matches
Functions
Amp
C » Controller » Data Record

Amp error statuses. More...

## Functions
bool | gclib_data_record_over_current (gclib_data_record_handle h, size_t amp)
| Returns over current status.
bool | gclib_data_record_over_voltage (gclib_data_record_handle h, size_t amp)
| Returns over voltage status.
bool | gclib_data_record_over_temp (gclib_data_record_handle h, size_t amp)
| Returns over temperature status.
bool | gclib_data_record_under_voltage (gclib_data_record_handle h, size_t amp)
| Returns under voltage status.
bool | gclib_data_record_electronic_lock_out (gclib_data_record_handle h, size_t amp)
| Returns electronic lockout (ELO) status for a bank.

## Detailed Description

Amp error statuses.

Amp errors are latched, and will need to be cleared with AZ once the underlying issue has been resolved. See the command reference for details.

## Function Documentation

## ◆ gclib_data_record_over_current()

bool gclib_data_record_over_current | ( | gclib_data_record_handle | h,
|  | size_t | amp )

Returns over current status.

## ◆ gclib_data_record_over_voltage()

bool gclib_data_record_over_voltage | ( | gclib_data_record_handle | h,
|  | size_t | amp )

Returns over voltage status.

## ◆ gclib_data_record_over_temp()

bool gclib_data_record_over_temp | ( | gclib_data_record_handle | h,
|  | size_t | amp )

Returns over temperature status.

## ◆ gclib_data_record_under_voltage()

bool gclib_data_record_under_voltage | ( | gclib_data_record_handle | h,
|  | size_t | amp )

Returns under voltage status.

## ◆ gclib_data_record_electronic_lock_out()

bool gclib_data_record_electronic_lock_out | ( | gclib_data_record_handle | h,
|  | size_t | amp )

Returns electronic lockout (ELO) status for a bank.