| gclib 1.34.15 Communications API for Galil controllers and PLCs |

## ◆ GInfo()

GReturn GCALL GInfo | ( | GCon | g,
|  | GCStringOut | info,
|  | GSize | info_len
| ) |  |

Uses GUtility() and G_UTIL_INFO to provide a useful connection string.

Parameters

  g | Connection's handle.
  info | Buffer to hold the output string. Buffer will be null terminated, even if the data must be truncated to do so.
  info_len | Length of buffer.

Returns
  The success status or error code of the function. See gclib_errors.h for possible values.

The response is address, revision_report, serial_number. For example:

    COM2, RIO47102 Rev 1.1j, 37290

See x_examples.cpp for an example.

Definition at line 49 of file gclibo.c.

References G_UTIL_INFO, and GUtility().