| gclib 1.34.15 Communications API for Galil controllers and PLCs |

Files | Macros | Typedefs | Functions
C++ examples

## Description

Files included in the C++ examples.

## Files
file | commands.cpp
file | commands_example.cpp
file | contour.cpp
file | contour_example.cpp
file | examples.h
file | ip_assigner.cpp
file | ip_assigner_example.cpp
file | jog.cpp
file | jog_example.cpp
file | message.cpp
file | message_example.cpp
file | motion_complete.cpp
file | motion_complete_example.cpp
file | position_tracking.cpp
file | position_tracking_example.cpp
file | record_position.cpp
file | record_position_example.cpp
file | remote_client.cpp
file | remote_server_example.cpp
file | remote_server.cpp
file | remote_server_example.cpp
file | vector.cpp
file | vector_example.cpp

## Macros
#define | _CRT_SECURE_NO_WARNINGS
#define | GALIL_EXAMPLE_OK 0
#define | GALIL_EXAMPLE_ERROR -100
#define | G_LASTINDEX 999

## Typedefs
typedef std::vector< string > | tokens

## Functions
GReturn | commands (GCon g)
| Demonstrates various uses of GCommand() and GUtility(). More...
int | main (int argc, char *argv[])
| Main function for Commands Example. More...
bool | load_buf (GCon g, const std::vector< int > &positions_A, const std::vector< int > &positions_B, int capacity, int &cmd)
| Loads contour buffer with commands from the given text file.
std::vector< int > | csv_to_vector (ifstream &is)
| Converts a file of comma separated values to a vector.
GReturn | contour (GCon g, char *fileA, char *fileB)
| Record user's training and plays back training through contour mode. More...
void | e (GReturn rc)
| A trivial, C++ style return code check used in Galil's examples and demos. More...
void | error (GCon g, GReturn rc)
| An example of error handling and debugging information.
int | pause ()
| Pauses console apps for a user key stroke.
GReturn | position_tracking (GCon g, int speed=5000)
| Puts controller into Position Tracking Mode and accepts user-entered positions. More...
GReturn | jog (GCon g)
| Puts controller into Jog Mode and accepts user input to adjust the speed. More...
GReturn | vector (GCon g, char *file)
| Puts controller into Vector Mode and accepts a file defining vector points. More...
GReturn | ip_assigner (char *serial_num, int address)
| Assigns controller an IP Adress given a serial number and a 1 byte address. More...
GReturn | motion_complete (GCon g)
| Uses interrupts to track when the motion of controller is completed. More...
GReturn | message (GCon g)
| Demonstrates how to receive messages from the controller and detect differences in Trace and crashed code. More...
GReturn | record_position (GCon g, char *fileA, char *fileB)
| Record user's training and saves to a text file. More...
GReturn | remote_server (const char *server_name)
| Publishes local gcaps server to the network. More...
GReturn | remote_client ()
| Lists available remote servers and allows connection to remote server. More...
tokens | string_split (const string &str, const string &token)
| Splits a string into a vector based on a token.
int | check_interrupts (GCon g, GCStringIn axes)
| Monitors interrupt status on the given axes and returns when interrupts are fired.
void | write_array_to_file (GCon g, ofstream &os, const char *array_name, int previous_rd, int rd)
| Grabs data from array on controller and writes it to the given text file.
void | print_client_message (const char *message)
void | print_servers_list (const std::vector< std::string > &server_list)
void | servers_to_list (std::vector< std::string > &server_list, std::string servers)
void | print_server_message (const char *message)
bool | load_buffer (GCon g, ifstream &fs, int capacity)