| gclib 1.34.15 Communications API for Galil controllers and PLCs |

Data Fields
GDataRecord Union Reference
API

Data record union, containing all structs and a generic byte array accessor. More...

`#include <gclib_record.h>`

## Data Fields
struct GDataRecord4000 | dmc4000
| The DMC-4000 data record.
struct GDataRecord4000 | dmc4103
| The DMC-4103 data record.
struct GDataRecord4000 | dmc50000
| The DMC-50000 data record.
struct GDataRecord52000 | dmc52000
| The DMC-52000 data record.
struct GDataRecord30000 | dmc30000
| The DMC-30000 data record.
struct GDataRecord2103 | dmc2103
| The DMC-21x3 data record.
struct GDataRecord1806 | dmc1806
| The DMC-1806 data record.
struct GDataRecord1802 | dmc1802
| The DMC-1802 data record.
struct GDataRecord47000_ENC | rio47000
| The RIO-471xx & 472xx data record, including encoder support.
struct GDataRecord47300_ENC | rio47300
| The RIO 473xx data record, including encoder support.
struct GDataRecord47300_24EX | rio47300_24ex
| The RIO 473xx data record, with 24EXOUT/24EXIN support.
struct GDataRecord47162 | rio47162
| The RIO 47162 data record.
unsigned char | byte_array [GALILDATARECORDMAXLENGTH]
| Generic byte array for offsets.

## Detailed Description

Data record union, containing all structs and a generic byte array accessor.

Named structs can be used to access typed data by name. Offsets into the data record can also be used by referencing the member `byte_array`.

//Getting the sample counter for the DMC-4000.
cout << data_record->dmc4000.sample_number << '\n'; //access by 4000 product
cout << * ((unsigned short *) (data_record->byte_array + 4)) << '\n'; //access by pointer arithmetic

Definition at line 1082 of file gclib_record.h.

The documentation for this union was generated from the following file:

- gclib_record.h