| gclib 2.0.7 Communications API for Galil controllers and PLCs |

## ◆ GMotionComplete()

void GMotionComplete | ( | string | axes | ) |
| inline

Blocking call that returns once all axes specified have completed their motion.

Parameters

  axes | A string containing a multiple-axes mask. Every character in the string should be a valid argument to MG_BGm, i.e. XYZWABCDEFGHST.

Wrapper around gclib GMotionComplete(), http://www.galil.com/sw/pub/all/doc/gclib/html/gclibo_8h.html#a19c220879442987970706444197f397a

Exceptions

  System.Exception | Will throw an exception if anything other than G_NO_ERROR is received from gclib.

Definition at line 428 of file gclib.cs.

Referenced by Examples.Contour(), Examples.Jog(), Examples.Position_Tracking(), and Examples.Vector_Mode().