| gclib 2.0.7 Communications API for Galil controllers and PLCs |

## ◆ GIpRequests()

String GIpRequests | ( |  | ) | throws GclibJavaException
| inline

Uses GUtility(), G_UTIL_GCAPS_IPREQUEST or G_UTIL_IPREQUEST to provide a list of all Galil controllers requesting IP addresses via BOOT-P or DHCP.

Returns
  String containing hardware requesting IP addresses.

DMC4000, 291, 00:50:4C:20:01:23, LAN, 10.1.3.10 RIO47000, 37290, 00:50:4C:28:91:AA, Static, 192.168.0.41

Exceptions

  GclibJavaException | If an error is generated by gclib.

Definition at line 449 of file GclibJava.java.