| gclib 2.0.7 Communications API for Galil controllers and PLCs |

## ◆ GOpen()

void GOpen | ( | string | address | ) |
| inline

Used to open a connection to Galil hardware.

Parameters

  address | Address string including any connection switches. See gclib documentation for GOpen().

Wrapper around gclib GOpen(), http://www.galil.com/sw/pub/all/doc/gclib/html/gclib_8h.html#aef4aec8a85630eed029b7a46aea7db54

Exceptions

  System.Exception | Will throw an exception if anything other than G_NO_ERROR is received from gclib.

Definition at line 445 of file gclib.cs.

Referenced by Examples.IP_Assigner(), Commands_Example.Main(), Contour_Example.Main(), Jog_Example.Main(), Message_Example.Main(), Motion_Complete_Example.Main(), Position_Tracking_Example.Main(), Record_Position_Example.Main(), and Vector_Mode_Example.Main().