| gclib 2.0.7 Communications API for Galil controllers and PLCs |

## ◆ GArrayUpload()

List<double> GArrayUpload | ( | string | array_name,
|  | Int16 | first = `-1`,
|  | Int16 | last = `-1`
| ) |  |
| inline

Uploads array data from the controller's array table.

Parameters

  array_name | String containing the name of the array to upload.
  first | The first element of the array for sub-array uploads.
  last | The last element of the array for sub-array uploads.

Returns
  The desired array as a list of doubles.

Wrapper around gclib GArrayUpload(), http://www.galil.com/sw/pub/all/doc/gclib/html/gclib_8h.html#af215806ec26ba06ed3f174ebeeafa7a7

Exceptions

  System.Exception | Will throw an exception if anything other than G_NO_ERROR is received from gclib.

Definition at line 173 of file gclib.cs.