| gclib 556 Communications API for Galil controllers and PLCs |

## ◆ Main()

static int Main | ( | string [] | args | ) |
| inline static

Main function for the contour example.

Parameters

  args | An array of command line arguments.

Returns
  The success status or error code of the function.

The first argument should be the IP Address of a Galil controller.
The second argument should be a path to a text file where training for Axis A will be recorded.
The third argument should be a path to a text file where training for Axis B will be recorded..

Definition at line 39 of file contour_example.cs.

References Examples.Contour(), Examples.GALIL_EXAMPLE_ERROR, Examples.GALIL_EXAMPLE_OK, and Examples.PrintError().